PCBNEW-BOARD Version 1 date 10/10/2011 12:25:29

# Created by Pcbnew(2010-05-05 BZR 2356)-stable

$GENERAL
LayerCount 2
Ly 1FFF8001
EnabledLayers 1FFF8001
Links 18
NoConn 0
Di 51776 27611 61610 34988
Ndraw 6
Ntrack 49
Nzone 0
BoardThickness 630
Nmodule 11
Nnets 8
$EndGENERAL

$SHEETDESCR
Sheet A4 11700 8267
Title ""
Date "10 oct 2011"
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndSHEETDESCR

$SETUP
InternalUnit 0.000100 INCH
ZoneGridSize 250
Layers 2
Layer[0] Dessous signal
Layer[15] Dessus signal
TrackWidth 80
TrackClearence 100
ZoneClearence 200
TrackMinWidth 80
DrawSegmWidth 150
EdgeSegmWidth 150
ViaSize 350
ViaDrill 250
ViaMinSize 350
ViaMinDrill 200
MicroViaSize 200
MicroViaDrill 50
MicroViasAllowed 0
MicroViaMinSize 200
MicroViaMinDrill 50
TextPcbWidth 120
TextPcbSize 600 800
EdgeModWidth 150
TextModSize 600 600
TextModWidth 120
PadSize 787 787
PadDrill 394
Pad2MaskClearance 100
AuxiliaryAxisOrg 0 0
$EndSETUP

$EQUIPOT
Na 0 ""
St ~
$EndEQUIPOT
$EQUIPOT
Na 1 "N-000001"
St ~
$EndEQUIPOT
$EQUIPOT
Na 2 "N-000002"
St ~
$EndEQUIPOT
$EQUIPOT
Na 3 "N-000003"
St ~
$EndEQUIPOT
$EQUIPOT
Na 4 "N-000004"
St ~
$EndEQUIPOT
$EQUIPOT
Na 5 "N-000006"
St ~
$EndEQUIPOT
$EQUIPOT
Na 6 "N-000007"
St ~
$EndEQUIPOT
$EQUIPOT
Na 7 "N-000008"
St ~
$EndEQUIPOT
$NCLASS
Name "Default"
Desc "Ceci est la Netclass par défaut"
Clearance 100
TrackWidth 80
ViaDia 350
ViaDrill 250
uViaDia 200
uViaDrill 50
AddNet ""
AddNet "N-000001"
AddNet "N-000002"
AddNet "N-000003"
AddNet "N-000004"
AddNet "N-000006"
AddNet "N-000007"
AddNet "N-000008"
$EndNCLASS
$MODULE LED-5MM
Po 53543 31299 2700 15 49BFA269 4E8D52AD ~~
Li LED-5MM
Cd LED 5mm - Lead pitch 100mil (2,54mm)
Kw LED led 5mm 5MM 100mil 2,54mm
Sc 4E8D52AD
AR /4E8B3321
Op 0 0 0
At VIRTUAL 
T0 0 -1500 300 300 2700 35 N V 21 N"D2"
T1 0 1500 300 300 2700 35 N V 21 N"1142581"
DS 1120 750 1120 -750 80 21
DC 100 0 -400 500 30 21
DA 100 0 1100 750 6462 100 21
DA 100 0 -350 0 4500 60 21
DA 100 0 550 0 4500 60 21
DA 100 0 -550 0 4500 60 21
DA 100 0 750 0 4500 60 21
DA 100 0 -750 0 4500 60 21
DA 100 0 950 0 4500 60 21
$PAD
Sh "1" C 660 660 0 0 2700
Dr 320 0 0
At STD N 00A8FFFF
Ne 6 "N-000007"
Po -500 0
$EndPAD
$PAD
Sh "2" C 660 660 0 0 2700
Dr 320 0 0
At STD N 00A8FFFF
Ne 7 "N-000008"
Po 500 0
$EndPAD
$SHAPE3D
Na "discret/leds/led5_vertical_verde.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  LED-5MM
$MODULE SM0805
Po 56299 29331 1800 15 42806E04 4E8D52AE ~~
Li SM0805
Sc 4E8D52AE
AR /4E8B342E
Op 0 0 0
At SMD 
T0 0 0 250 250 1800 50 N V 21 N"C1"
T1 0 0 250 250 1800 50 N I 21 N"100n"
DC -650 300 -650 250 50 21
DS -200 300 -600 300 50 21
DS -600 300 -600 -300 50 21
DS -600 -300 -200 -300 50 21
DS 200 -300 600 -300 50 21
DS 600 -300 600 300 50 21
DS 600 300 200 300 50 21
$PAD
Sh "1" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 5 "N-000006"
Po -375 0
$EndPAD
$PAD
Sh "2" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 7 "N-000008"
Po 375 0
$EndPAD
$SHAPE3D
Na "smd/chip_cms.wrl"
Sc 0.100000 0.100000 0.100000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  SM0805
$MODULE SM0805
Po 55118 31299 1800 15 42806E04 4E8D52B0 ~~
Li SM0805
Sc 4E8D52B0
AR /4E8B341A
Op 0 0 0
At SMD 
T0 0 0 250 250 1800 50 N V 21 N"R4"
T1 0 0 250 250 1800 50 N I 21 N"68"
DC -650 300 -650 250 50 21
DS -200 300 -600 300 50 21
DS -600 300 -600 -300 50 21
DS -600 -300 -200 -300 50 21
DS 200 -300 600 -300 50 21
DS 600 -300 600 300 50 21
DS 600 300 200 300 50 21
$PAD
Sh "1" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 1 "N-000001"
Po -375 0
$EndPAD
$PAD
Sh "2" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 6 "N-000007"
Po 375 0
$EndPAD
$SHAPE3D
Na "smd/chip_cms.wrl"
Sc 0.100000 0.100000 0.100000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  SM0805
$MODULE SM0805
Po 57283 33268 1800 15 42806E04 4E8D52B2 ~~
Li SM0805
Sc 4E8D52B2
AR /4E8B3412
Op 0 0 0
At SMD 
T0 0 0 250 250 1800 50 N V 21 N"R5"
T1 0 0 250 250 1800 50 N I 21 N"1M"
DC -650 300 -650 250 50 21
DS -200 300 -600 300 50 21
DS -600 300 -600 -300 50 21
DS -600 -300 -200 -300 50 21
DS 200 -300 600 -300 50 21
DS 600 -300 600 300 50 21
DS 600 300 200 300 50 21
$PAD
Sh "1" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 3 "N-000003"
Po -375 0
$EndPAD
$PAD
Sh "2" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 4 "N-000004"
Po 375 0
$EndPAD
$SHAPE3D
Na "smd/chip_cms.wrl"
Sc 0.100000 0.100000 0.100000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  SM0805
$MODULE SM0805
Po 57874 29331 1800 15 42806E04 4E8D52B4 ~~
Li SM0805
Sc 4E8D52B4
AR /4E8B340E
Op 0 0 0
At SMD 
T0 0 0 250 250 1800 50 N V 21 N"R1"
T1 0 0 250 250 1800 50 N I 21 N"3M"
DC -650 300 -650 250 50 21
DS -200 300 -600 300 50 21
DS -600 300 -600 -300 50 21
DS -600 -300 -200 -300 50 21
DS 200 -300 600 -300 50 21
DS 600 -300 600 300 50 21
DS 600 300 200 300 50 21
$PAD
Sh "1" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 3 "N-000003"
Po -375 0
$EndPAD
$PAD
Sh "2" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 5 "N-000006"
Po 375 0
$EndPAD
$SHAPE3D
Na "smd/chip_cms.wrl"
Sc 0.100000 0.100000 0.100000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  SM0805
$MODULE SM0805
Po 54724 32874 900 15 42806E04 4E8D52B6 ~~
Li SM0805
Sc 4E8D52B6
AR /4E8B3416
Op 0 0 0
At SMD 
T0 0 0 250 250 900 50 N V 21 N"R2"
T1 0 0 250 250 900 50 N I 21 N"10k"
DC -650 300 -650 250 50 21
DS -200 300 -600 300 50 21
DS -600 300 -600 -300 50 21
DS -600 -300 -200 -300 50 21
DS 200 -300 600 -300 50 21
DS 600 -300 600 300 50 21
DS 600 300 200 300 50 21
$PAD
Sh "1" R 350 550 0 0 900
Dr 0 0 0
At SMD N 00888000
Ne 2 "N-000002"
Po -375 0
$EndPAD
$PAD
Sh "2" R 350 550 0 0 900
Dr 0 0 0
At SMD N 00888000
Ne 7 "N-000008"
Po 375 0
$EndPAD
$SHAPE3D
Na "smd/chip_cms.wrl"
Sc 0.100000 0.100000 0.100000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  SM0805
$MODULE SM0805
Po 55906 33268 1800 15 42806E04 4E8D52B8 ~~
Li SM0805
Sc 4E8D52B8
AR /4E8B3429
Op 0 0 0
At SMD 
T0 0 0 250 250 1800 50 N V 21 N"C2"
T1 0 0 250 250 1800 50 N I 21 N"100n"
DC -650 300 -650 250 50 21
DS -200 300 -600 300 50 21
DS -600 300 -600 -300 50 21
DS -600 -300 -200 -300 50 21
DS 200 -300 600 -300 50 21
DS 600 -300 600 300 50 21
DS 600 300 200 300 50 21
$PAD
Sh "1" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 4 "N-000004"
Po -375 0
$EndPAD
$PAD
Sh "2" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 2 "N-000002"
Po 375 0
$EndPAD
$SHAPE3D
Na "smd/chip_cms.wrl"
Sc 0.100000 0.100000 0.100000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  SM0805
$MODULE SO8E
Po 57087 31299 0 15 42806F54 4E8D52B9 ~~
Li SO8E
Cd module CMS SOJ 8 pins etroit
Kw CMS SOJ
Sc 4E8D52B9
AR /4E8B33ED
Op 0 0 0
At SMD 
T0 0 -350 450 450 0 60 N V 21 N"U1"
T1 0 400 350 350 0 60 N V 21 N"NE555"
DS -1050 700 -1050 750 50 21
DS -1050 750 1050 750 50 21
DS 1050 -750 -1050 -750 50 21
DS -1050 -750 -1050 700 50 21
DS -1050 -200 -850 -200 50 21
DS -850 -200 -850 200 50 21
DS -850 200 -1050 200 50 21
DS 1050 -750 1050 750 50 21
$PAD
Sh "8" R 200 450 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 3 "N-000003"
Po -750 -1050
$EndPAD
$PAD
Sh "1" R 200 450 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 7 "N-000008"
Po -750 1050
$EndPAD
$PAD
Sh "7" R 200 450 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 5 "N-000006"
Po -250 -1050
$EndPAD
$PAD
Sh "6" R 200 450 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 5 "N-000006"
Po 250 -1050
$EndPAD
$PAD
Sh "5" R 200 450 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 0 ""
Po 750 -1050
$EndPAD
$PAD
Sh "2" R 200 450 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 4 "N-000004"
Po -250 1050
$EndPAD
$PAD
Sh "3" R 200 450 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 1 "N-000001"
Po 250 1050
$EndPAD
$PAD
Sh "4" R 200 450 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 3 "N-000003"
Po 750 1050
$EndPAD
$SHAPE3D
Na "smd/cms_so8.wrl"
Sc 0.500000 0.320000 0.500000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  SO8E
$MODULE LED-5MM
Po 59843 31299 900 15 49BFA269 4E8D6CC2 ~~
Li LED-5MM
Cd LED 5mm - Lead pitch 100mil (2,54mm)
Kw LED led 5mm 5MM 100mil 2,54mm
Sc 4E8D6CC2
AR /4E8D6BD0
Op 0 0 0
At VIRTUAL 
T0 0 -1500 300 300 900 35 N V 21 N"D1"
T1 0 1500 300 300 900 35 N V 21 N"1497676"
DS 1120 750 1120 -750 80 21
DC 100 0 -400 500 30 21
DA 100 0 1100 750 6462 100 21
DA 100 0 -350 0 4500 60 21
DA 100 0 550 0 4500 60 21
DA 100 0 -550 0 4500 60 21
DA 100 0 750 0 4500 60 21
DA 100 0 -750 0 4500 60 21
DA 100 0 950 0 4500 60 21
$PAD
Sh "1" C 660 660 0 0 900
Dr 320 0 0
At STD N 00A8FFFF
Ne 2 "N-000002"
Po -500 0
$EndPAD
$PAD
Sh "2" C 660 660 0 0 900
Dr 320 0 0
At STD N 00A8FFFF
Ne 3 "N-000003"
Po 500 0
$EndPAD
$SHAPE3D
Na "discret/leds/led5_vertical_verde.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  LED-5MM
$MODULE 1_PIN
Po 59843 29134 0 15 4E8D6EC1 4E8D709D ~~
Li 1_PIN
Sc 4E8D709D
AR /4E8B351E
Op 0 0 0
T0 0 -1063 600 600 0 120 N V 21 N"P1"
T1 0 1063 600 600 0 120 N V 21 N"3V"
$PAD
Sh "1" C 787 787 0 0 0
Dr 394 0 0
At STD N 00E0FFFF
Ne 3 "N-000003"
Po 0 0
$EndPAD
$EndMODULE  1_PIN
$MODULE 1_PIN
Po 53543 33465 0 15 4E8D6EC1 4E8D709F ~~
Li 1_PIN
Sc 4E8D709F
AR /4E8B3525
Op 0 0 0
T0 0 -1063 600 600 0 120 N V 21 N"P2"
T1 0 1063 600 600 0 120 N V 21 N"GND"
$PAD
Sh "1" C 787 787 0 0 0
Dr 394 0 0
At STD N 00E0FFFF
Ne 7 "N-000008"
Po 0 0
$EndPAD
$EndMODULE  1_PIN
$DRAWSEGMENT
Po 0 52756 34252 52756 28346 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 60630 28346 60630 34252 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$COTATION
Ge 0 28 0
Va 5906
Te "15.001 mm"
Po 50542 31299 600 800 120 2700 1
Sb 0 51182 28346 51182 34252 120
Sd 0 51969 34252 49902 34252 120
Sg 0 51969 28346 49902 28346 120
S1 0 51182 34252 50952 33809 120
S2 0 51182 34252 51412 33809 120
S3 0 51182 28346 50952 28789 120
S4 0 51182 28346 51412 28789 120
$endCOTATION
$DRAWSEGMENT
Po 0 60630 28346 52756 28346 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 52756 34252 60630 34252 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$COTATION
Ge 0 28 0
Va 7874
Te "20.000 mm"
Po 56693 36072 600 800 120 0 1
Sb 0 52756 35432 60630 35432 120
Sd 0 60630 34646 60630 36712 120
Sg 0 52756 34646 52756 36712 120
S1 0 60630 35432 60187 35662 120
S2 0 60630 35432 60187 35202 120
S3 0 52756 35432 53199 35662 120
S4 0 52756 35432 53199 35202 120
$endCOTATION
$TRACK
Po 0 55494 31300 55493 31299 80 -1
De 15 0 1 0 400
Po 0 57086 31300 55494 31300 80 -1
De 15 0 1 0 0
Po 0 57337 31551 57086 31300 80 -1
De 15 0 1 0 0
Po 0 57337 32349 57337 31551 80 -1
De 15 0 1 0 800
Po 0 55531 33680 55531 33268 80 -1
De 15 0 2 0 400
Po 0 55709 33858 55531 33680 80 -1
De 15 0 2 0 0
Po 0 58071 33858 55709 33858 80 -1
De 15 0 2 0 0
Po 0 58268 33661 58071 33858 80 -1
De 15 0 2 0 0
Po 0 58268 32087 58268 33661 80 -1
De 15 0 2 0 0
Po 0 58556 31799 58268 32087 80 -1
De 15 0 2 0 0
Po 0 54743 33268 54724 33249 80 -1
De 15 0 2 0 400
Po 0 55531 33268 54743 33268 80 -1
De 15 0 2 0 800
Po 0 59843 31799 58556 31799 80 -1
De 15 0 2 0 800
Po 0 58249 29331 58858 29331 80 -1
De 15 0 3 0 800
Po 0 58858 29134 58858 29134 80 -1
De 15 0 3 0 0
Po 0 58858 29134 58858 29331 80 -1
De 15 0 3 0 0
Po 0 58858 29331 58858 30799 80 -1
De 15 0 3 0 0
Po 0 56337 30747 56389 30799 80 -1
De 15 0 3 0 0
Po 0 56389 30799 57837 30799 80 -1
De 15 0 3 0 0
Po 0 57837 30799 58858 30799 80 -1
De 15 0 3 0 0
Po 0 58858 30799 59843 30799 80 -1
De 15 0 3 0 400
Po 0 57837 32349 57837 33089 80 -1
De 15 0 3 0 800
Po 0 57837 33089 57658 33268 80 -1
De 15 0 3 0 400
Po 0 57837 32349 57837 30799 80 -1
De 15 0 3 0 800
Po 0 56337 30249 56337 30747 80 -1
De 15 0 3 0 800
Po 0 59843 29134 58858 29134 80 -1
De 15 0 3 0 800
Po 0 56908 33268 56281 33268 80 -1
De 15 0 4 0 C00
Po 0 56837 32349 56837 33197 80 -1
De 15 0 4 0 800
Po 0 56837 33197 56908 33268 80 -1
De 15 0 4 0 400
Po 0 57087 30249 57087 29331 80 -1
De 15 0 5 0 0
Po 0 56674 29331 57087 29331 80 -1
De 15 0 5 0 800
Po 0 57087 29331 57499 29331 80 -1
De 15 0 5 0 400
Po 0 57337 30249 57087 30249 80 -1
De 15 0 5 0 800
Po 0 57087 30249 56837 30249 80 -1
De 15 0 5 0 400
Po 0 54743 31299 54330 31299 80 -1
De 15 0 6 0 800
Po 0 53830 30799 53543 30799 80 -1
De 15 0 6 0 400
Po 0 54330 31299 53830 30799 80 -1
De 15 0 6 0 0
Po 0 55924 29331 55315 29331 80 -1
De 15 0 7 0 800
Po 0 55118 29528 55118 32499 80 -1
De 15 0 7 0 0
Po 0 55315 29331 55118 29528 80 -1
De 15 0 7 0 0
Po 0 55099 32499 55118 32499 80 -1
De 15 0 7 0 0
Po 0 55118 32499 56280 32499 80 -1
De 15 0 7 0 0
Po 0 56299 32480 56337 32349 80 -1
De 15 0 7 0 400
Po 0 56280 32499 56299 32480 80 -1
De 15 0 7 0 0
Po 0 55099 32499 54724 32499 80 -1
De 15 0 7 0 400
Po 0 53543 33465 53543 31799 80 -1
De 15 0 7 0 C00
Po 0 54724 32499 53562 32499 80 -1
De 15 0 7 0 800
Po 0 53543 32480 53543 31799 80 -1
De 15 0 7 0 400
Po 0 53562 32499 53543 32480 80 -1
De 15 0 7 0 0
$EndTRACK
$ZONE
$EndZONE
$EndBOARD
